# Future Evidence Register

## FEVID-001 — GCC-4241N A100/A101 TSOP Transform

**Status:** Resolved for the transform.

The exact XOR and GCC bit permutation are validated for accurate A100 and A101
dumps. Checksum and stock updater transform location remain open.

## FEVID-002 — Failed A101 Flash Attempt

**Status:** Partially resolved.

The failed image is plaintext A101 outside a preserved 16 KiB window. The
packaged log is contextual but not proven to describe the same attempt.
