# GCC-4244N Batch-07 Current Evidence Summary

## Preserved evidence

- historical GCC-4244N research HTML;
- current `stage5b_0024` device profile;
- all current `stage5b_0024` findings rows.

## Current analyzer state

- normalized firmware base: `0x90000000`
- recipient status: `strong_recipient_candidate`
- recipient score: `82.78`
- READ DVD STRUCTURE `0xAD`: present, tier `table_entry_valid`
- required command surface: complete as static analyzer evidence
- vendor `0xE7`: recognized
- verified `AD/C0` Xbox-auth payload handler: **not present**
- parser gate: `0x900386FB`, CDB base `0x894`
- parser tokens: `HL`, `IT`, `RPC`, `RPC_JCS3`, `RPC_SUFFIX`
- parser smoke validation exists, but `live_safe=false`
- code-cave candidate total: 141,857 bytes across six runs

These findings make GCC-4244N 104 a strong research recipient candidate. They do not prove that historical hook addresses are correct, that the flash stub is safe, or that Xbox functions are ready for injection.

## Revision boundary

The historical report calls its target `B104`. Current analyzer artifacts identify `104`, while the current user fleet is expected to run `VB104`. These provenance labels must remain distinct until exact image lineage is established.
