# PFES-MIG-003 Completion Report — Current Emulator Knowledge Migration

**PFES revision:** 0.14.0  
**Completed:** 2026-07-13T02:24:40.851996+00:00

## Scope closed

PFES now preserves:

- v206 known-good behavioral baseline;
- exact v258 package and exact v258 live-artifact archive;
- component and source inventories;
- all-Python compile validation and fast CPU flag regression;
- READ(10) parser/descriptor state-handoff closure;
- explicit seeded, state-handoff, uninterrupted-execution, bridge-model, and
  hardware proof boundaries;
- current media-window delta status;
- timer/MMIO negative knowledge;
- device/media/session/proof/test ownership;
- Windows iSCSI, logging, test, and package contracts.

## Exact archives

```text
mn103s_emu_v258.zip
SHA-256 8915ca24b760437007de3f1ab6b96c8f5ebd63bead40410d3e211e134c240563

gdr8050l_auth_v258_dynamic_iscsi_live_artifacts.zip
SHA-256 ea9d16883422738a747a840f5c450bbe1cc0591f7fdf4be070d6cf5c6a436d31
```

## Local validation

- Python source files compiled: 27 / 27
- MN103S flag regression: pass
- Long emulator rerun performed: no
- Live artifact core reports validated: yes

## Current closed/open boundary

Closed:

- READ(10) natural front dispatch and handler;
- firmware-derived host LBA;
- parser/descriptor state handoff;
- phase-4 descriptor consumer.

Open:

- single uninterrupted call stack;
- READ(12) equivalent closure;
- descriptor-output/window consumer;
- firmware-derived 198,144-sector delta;
- exact timer/MMIO behavior.

## Next PFES task

`PFES-MAINT-003` — normalize claims and cross-references across the historical,
analyzer, emulator, media, device, and operating-contract records.
